Plot Report
-----------

Report Written:     Tuesday, March 12, 2019
Design Path:        H:\PrimerCube Tech Transfer\Printed Circuit Boards\PC DC Input Mini PCB.pcb
Design Title:       
Created:            5/23/2015 4:29:52 PM
Last Saved:         3/12/2019 4:54:02 PM
Editing Time:       1059 min
Units:              thou (precision 0)


Device Settings
===============


Gerber Settings
===============

    Leading zero suppression.
    G01 assumed throughout.
    Line termination <*> <CR> <LF>.
    3.5 format absolute inches.

    Format commands defined in Gerber file.
    Aperture table defined in Gerber file.
    Hardware arcs allowed.


Drill Settings
==============

    Excellon Format 1    Format 3.5 absolute in mm.
    Zero suppression Leading



Plots Output
============

    Plot Job: "H:\PrimerCube Tech Transfer\Printed Circuit Boards\PC DC Input Mini PCB.mop"


Gerber Output
=============

H:\PrimerCube Tech Transfer\Printed Circuit Boards\PC DC Input Mini PCB - Top Silkscreen.gbr

    Layers:
    ------------------
    Top Silkscreen
    Board Outlines

    D-Code Shape  (thou)
    -----------------------
    D28    Round 5.00

Gerber Output
=============

H:\PrimerCube Tech Transfer\Printed Circuit Boards\PC DC Input Mini PCB - Top Copper.gbr

    Layers:
    --------------
    Top Copper

    D-Code Shape  (thou)
    ----------------------------------
    D29    Round 125.00
    D72    Rectangle 50.00 X 100.00
    D73    Rectangle 39.37 X 137.80
    D74    Rectangle 59.06 X 137.80
    D75    Round 25.00
    D76    Round 50.00

Gerber Output
=============

H:\PrimerCube Tech Transfer\Printed Circuit Boards\PC DC Input Mini PCB - Top Copper (Resist).gbr

    Layers:
    --------------
    Top Copper

    D-Code Shape  (thou)
    ----------------------------------
    D77    Round 135.00
    D78    Rectangle 60.00 X 110.00
    D79    Rectangle 49.37 X 147.80
    D80    Rectangle 69.06 X 147.80

Gerber Output
=============

H:\PrimerCube Tech Transfer\Printed Circuit Boards\PC DC Input Mini PCB - Top Copper (Paste).gbr

    Layers:
    --------------
    Top Copper

    D-Code Shape  (thou)
    ----------------------------------
    D81    Rectangle 46.00 X 96.00
    D82    Rectangle 35.37 X 133.80
    D83    Rectangle 55.06 X 133.80

Gerber Output
=============

H:\PrimerCube Tech Transfer\Printed Circuit Boards\PC DC Input Mini PCB - Bottom Copper.gbr

    Layers:
    -----------------
    Bottom Copper

    D-Code Shape  (thou)
    -----------------------
    D29    Round 125.00

Gerber Output
=============

H:\PrimerCube Tech Transfer\Printed Circuit Boards\PC DC Input Mini PCB - Bottom Copper (Resist).gbr

    Layers:
    -----------------
    Bottom Copper

    D-Code Shape  (thou)
    -----------------------
    D77    Round 135.00

Gerber Output
=============

H:\PrimerCube Tech Transfer\Printed Circuit Boards\PC DC Input Mini PCB - Bottom Copper (Paste).gbr

    Layers:
    -----------------
    Bottom Copper

    D-Code Shape  (thou)
    -----------------------

NC Drill Output
===============

H:\PrimerCube Tech Transfer\Printed Circuit Boards\PC DC Input Mini PCB - Drill Data - Through Hole.drl

    Output:
    ---------------------------
    Plated Round Drill Holes
    Plated Slots
    Plated Board Outlines

    Tool  Size           Count   ID
    --------------------------------------
    T001  0.12000 inches 1     F
    --------------------------------------
    Total                1
    --------------------------------------

H:\PrimerCube Tech Transfer\Printed Circuit Boards\PC DC Input Mini PCB - Drill Data - Through Hole (Unplated).drl

    Output:
    -----------------------------
    Unplated Round Drill Holes
    Unplated Slots
    Unplated Board Outlines

    Tool  Size           Count   ID
    --------------------------------------
    T001  0.02500 inches 1
    --------------------------------------
    Total                1
    --------------------------------------


Gerber Output
=============

H:\PrimerCube Tech Transfer\Printed Circuit Boards\PC DC Input Mini PCB - Drill Ident Drawing - Through Hole.gbr

    Layers:
    ------------------
    [Through Hole]


Drill Ident Drawing
===================

    Drill Plated Size Shape ID
    -----------------------------------
    120   Y      100  Round F

    D-Code Shape  (thou)
    -----------------------
    D27    Round 100.00
    D28    Round 5.00

End Of Report.
