File PC Bowl V10.NC.tap

This file was compiled for a small 5 axis CNC mill.(Shown in photo in this folder with the five axis labeled)

Compressed air was use to continously remove chips and cool the cutting bit but the air compressor was undersized therefore delays were added to allow the air compressor to "catch up"

With a larger air compressor source this delay can be removed or reduced.

