Plot Report
-----------

Report Written:     Tuesday, March 12, 2019
Project Path:       H:\PrimerCube Tech Transfer\Printed Circuit Boards\PC CMB Aux PCB v8.prj
Design Path:        H:\PrimerCube Tech Transfer\Printed Circuit Boards\PC CMB Aux PCB v8.pcb
Design Title:       
Created:            5/12/2015 3:17:50 PM
Last Saved:         7/30/2015 12:36:48 PM
Editing Time:       30925 min
Units:              thou (precision 0)


Device Settings
===============


Gerber Settings
===============

    Leading zero suppression.
    G01 assumed throughout.
    Line termination <*> <CR> <LF>.
    3.5 format absolute inches.

    Format commands defined in Gerber file.
    Aperture table defined in Gerber file.
    Hardware arcs allowed.


Drill Settings
==============

    Excellon Format 1    Format 3.5 absolute in mm.
    Zero suppression Leading



Plots Output
============

    Plot Job: "H:\PrimerCube Tech Transfer\Printed Circuit Boards\PC CMB Aux PCB v8.mop"


Gerber Output
=============

H:\PrimerCube Tech Transfer\Printed Circuit Boards\PC CMB Aux PCB v8 - Top Documentation.gbr

    Layers:
    ---------------------
    Top Documentation
    Board Outlines

    D-Code Shape  (thou)
    -----------------------
    D10    Round 1.00
    D11    Round 5.00

Gerber Output
=============

H:\PrimerCube Tech Transfer\Printed Circuit Boards\PC CMB Aux PCB v8 - Top Silkscreen.gbr

    Layers:
    ------------------
    Top Silkscreen
    Board Outlines

    D-Code Shape  (thou)
    -----------------------
    D10    Round 1.00
    D11    Round 5.00
    D12    Round 10.00
    D13    Round 6.00
    D14    Round 3.00

Gerber Output
=============

H:\PrimerCube Tech Transfer\Printed Circuit Boards\PC CMB Aux PCB v8 - Top Copper.gbr

    Layers:
    --------------
    Top Copper

    D-Code Shape  (thou)
    -----------------------------------------------
    D15    Rectangle 50.00 X 100.00  Rotation 90
    D16    Square 200.00
    D17    Rectangle 15.75 X 47.24  Rotation 90
    D18    Rectangle 39.37 X 42.91
    D19    Rectangle 20.00 X 53.00  Rotation 90
    D70    Rectangle 80.00 X 190.00  Rotation 90
    D71    Rectangle 31.00 X 149.00  Rotation 90
    D20    Rectangle 71.00 X 86.00
    D21    Rectangle 40.00 X 120.00  Rotation 90
    D22    Rectangle 330.00 X 420.00
    D23    Rectangle 39.37 X 42.91  Rotation 90
    D24    Round 50.00
    D25    Round 25.00
    D26    Round 32.00
    D27    Round 48.00
    D28    Round 15.00
    D29    Round 35.00
    D72    Round 56.00

Gerber Output
=============

H:\PrimerCube Tech Transfer\Printed Circuit Boards\PC CMB Aux PCB v8 - Top Solder Mask.gbr

    Layers:
    -------------------
    Top Solder Mask

    D-Code Shape  (thou)
    -----------------------------------------------
    D73    Rectangle 56.00 X 106.00  Rotation 90
    D74    Square 206.00
    D75    Rectangle 21.75 X 53.24  Rotation 90
    D76    Rectangle 45.37 X 48.91
    D77    Rectangle 26.00 X 59.00  Rotation 90
    D78    Rectangle 86.00 X 196.00  Rotation 90
    D79    Rectangle 37.00 X 155.00  Rotation 90
    D80    Rectangle 77.00 X 92.00
    D81    Rectangle 46.00 X 126.00  Rotation 90
    D82    Rectangle 336.00 X 426.00
    D83    Rectangle 45.37 X 48.91  Rotation 90
    D84    Round 38.00
    D85    Round 54.00
    D86    Round 62.00

Gerber Output
=============

H:\PrimerCube Tech Transfer\Printed Circuit Boards\PC CMB Aux PCB v8 - Top Paste Mask.gbr

    Layers:
    ------------------
    Top Paste Mask

    D-Code Shape  (thou)
    -----------------------------------------------
    D87    Rectangle 44.00 X 94.00  Rotation 90
    D88    Square 194.00
    D89    Rectangle 9.75 X 41.24  Rotation 90
    D90    Rectangle 33.37 X 36.91
    D91    Rectangle 14.00 X 47.00  Rotation 90
    D92    Rectangle 74.00 X 184.00  Rotation 90
    D93    Rectangle 25.00 X 143.00  Rotation 90
    D94    Rectangle 65.00 X 80.00
    D95    Rectangle 34.00 X 114.00  Rotation 90
    D96    Rectangle 324.00 X 414.00
    D97    Rectangle 33.37 X 36.91  Rotation 90

Gerber Output
=============

H:\PrimerCube Tech Transfer\Printed Circuit Boards\PC CMB Aux PCB v8 - Bottom Copper.gbr

    Layers:
    -----------------
    Bottom Copper

    D-Code Shape  (thou)
    -----------------------
    D24    Round 50.00
    D25    Round 25.00
    D26    Round 32.00
    D27    Round 48.00
    D72    Round 56.00

Gerber Output
=============

H:\PrimerCube Tech Transfer\Printed Circuit Boards\PC CMB Aux PCB v8 - Bottom Solder Mask.gbr

    Layers:
    ----------------------
    Bottom Solder Mask

    D-Code Shape  (thou)
    -----------------------
    D84    Round 38.00
    D85    Round 54.00
    D86    Round 62.00

Gerber Output
=============

H:\PrimerCube Tech Transfer\Printed Circuit Boards\PC CMB Aux PCB v8 - Bottom Paste Mask.gbr

    Layers:
    ---------------------
    Bottom Paste Mask

    D-Code Shape  (thou)
    -----------------------

NC Drill Output
===============

H:\PrimerCube Tech Transfer\Printed Circuit Boards\PC CMB Aux PCB v8 - Drill Data - Through Hole.drl

    Output:
    ---------------------------
    Plated Round Drill Holes
    Plated Slots
    Plated Board Outlines

    Tool  Size           Count   ID
    --------------------------------------
    T001  0.01600 inches 1     A
    T002  0.02400 inches 13    B
    T003  0.03200 inches 4     C
    --------------------------------------
    Total                18
    --------------------------------------

H:\PrimerCube Tech Transfer\Printed Circuit Boards\PC CMB Aux PCB v8 - Drill Data - Through Hole (Unplated).drl

    Output:
    -----------------------------
    Unplated Round Drill Holes
    Unplated Slots
    Unplated Board Outlines

    Tool  Size           Count   ID
    --------------------------------------
    T001  0.02500 inches 1
    --------------------------------------
    Total                1
    --------------------------------------


Gerber Output
=============

H:\PrimerCube Tech Transfer\Printed Circuit Boards\PC CMB Aux PCB v8 - Drill Ident Drawing - Through Hole.gbr

    Layers:
    ------------------
    [Through Hole]


Drill Ident Drawing
===================

    Drill Plated Size Shape ID
    -----------------------------------
    16    Y      100  Round A
    24    Y      100  Round B
    32    Y      100  Round C

    D-Code Shape  (thou)
    -----------------------
    D11    Round 5.00
    D98    Round 100.00

End Of Report.
