Plot Report
-----------

Report Written:     Tuesday, March 12, 2019
Project Path:       H:\PrimerCube Tech Transfer\Printed Circuit Boards\PC MotherBoard v10.prj
Design Path:        H:\PrimerCube Tech Transfer\Printed Circuit Boards\PrimerCube MotherBoard V10.pcb
Design Title:       
Created:            4/10/2015 11:08:49 AM
Last Saved:         3/12/2019 4:27:37 PM
Editing Time:       38198 min
Units:              thou (precision 0)


Device Settings
===============


Gerber Settings
===============

    Leading zero suppression.
    G01 assumed throughout.
    Line termination <*> <CR> <LF>.
    3.5 format absolute inches.

    Format commands defined in Gerber file.
    Aperture table defined in Gerber file.
    Hardware arcs allowed.


Drill Settings
==============

    Excellon Format 1    Format 3.5 absolute in mm.
    Zero suppression Leading



Plots Output
============

    Plot Job: "H:\PrimerCube Tech Transfer\Printed Circuit Boards\PrimerCube MotherBoard V10.mop"


Gerber Output
=============

H:\PrimerCube Tech Transfer\Printed Circuit Boards\PrimerCube MotherBoard V10 - Top Documentation.gbr

    Layers:
    ---------------------
    Top Documentation
    Board Outlines

    D-Code Shape  (thou)
    -----------------------
    D10    Round 1.00
    D11    Round 5.00

Gerber Output
=============

H:\PrimerCube Tech Transfer\Printed Circuit Boards\PrimerCube MotherBoard V10 - Top Silkscreen.gbr

    Layers:
    ------------------
    Top Silkscreen
    Board Outlines

    D-Code Shape  (thou)
    -----------------------
    D10    Round 1.00
    D11    Round 5.00
    D13    Round 6.00
    D14    Round 3.00

Gerber Output
=============

H:\PrimerCube Tech Transfer\Printed Circuit Boards\PrimerCube MotherBoard V10 - Top Copper.gbr

    Layers:
    --------------
    Top Copper

    D-Code Shape  (thou)
    -----------------------------------------------
    D12    Round 10.00
    D18    Rectangle 39.37 X 42.91
    D24    Round 50.00
    D25    Round 25.00
    D26    Round 32.00
    D27    Round 48.00
    D28    Round 15.00
    D72    Round 56.00
    D99    Square 54.00
    D100   Round 54.00
    D101   Round 70.00
    D102   Rectangle 22.00 X 74.80  Rotation 90
    D103   Rectangle 100.39 X 110.24
    D104   Rectangle 23.62 X 78.74
    D105   Rectangle 15.94 X 38.98
    D106   Rectangle 90.55 X 98.43
    D107   Rectangle 15.75 X 47.24
    D108   Rectangle 39.37 X 137.80  Rotation 90
    D109   Rectangle 59.06 X 137.80  Rotation 90
    D110   Rectangle 69.00 X 87.00
    D111   Square 60.00
    D112   Round 60.00
    D113   Rectangle 26.00 X 41.00
    D114   Rectangle 40.00 X 48.00
    D115   Round 20.00

Gerber Output
=============

H:\PrimerCube Tech Transfer\Printed Circuit Boards\PrimerCube MotherBoard V10 - Top Solder Mask.gbr

    Layers:
    -------------------
    Top Solder Mask

    D-Code Shape  (thou)
    -----------------------------------------------
    D76    Rectangle 45.37 X 48.91
    D116   Square 60.00
    D117   Round 60.00
    D118   Round 76.00
    D119   Rectangle 28.00 X 80.80  Rotation 90
    D120   Rectangle 106.39 X 116.24
    D121   Rectangle 29.62 X 84.74
    D122   Rectangle 21.94 X 44.98
    D123   Rectangle 96.55 X 104.43
    D124   Rectangle 21.75 X 53.24
    D125   Rectangle 45.37 X 143.80  Rotation 90
    D126   Rectangle 65.06 X 143.80  Rotation 90
    D127   Rectangle 75.00 X 93.00
    D128   Square 66.00
    D129   Round 66.00
    D130   Rectangle 32.00 X 47.00
    D131   Rectangle 46.00 X 54.00

Gerber Output
=============

H:\PrimerCube Tech Transfer\Printed Circuit Boards\PrimerCube MotherBoard V10 - Top Paste Mask.gbr

    Layers:
    ------------------
    Top Paste Mask

    D-Code Shape  (thou)
    -----------------------------------------------
    D90    Rectangle 33.37 X 36.91
    D132   Rectangle 16.00 X 68.80  Rotation 90
    D133   Rectangle 94.39 X 104.24
    D134   Rectangle 17.62 X 72.74
    D135   Rectangle 9.94 X 32.98
    D136   Rectangle 84.55 X 92.43
    D137   Rectangle 9.75 X 41.24
    D138   Rectangle 33.37 X 131.80  Rotation 90
    D139   Rectangle 53.06 X 131.80  Rotation 90
    D140   Rectangle 63.00 X 81.00
    D141   Rectangle 20.00 X 35.00
    D142   Rectangle 34.00 X 42.00

Gerber Output
=============

H:\PrimerCube Tech Transfer\Printed Circuit Boards\PrimerCube MotherBoard V10 - Bottom Copper.gbr

    Layers:
    -----------------
    Bottom Copper

    D-Code Shape  (thou)
    ------------------------------------------------
    D12    Round 10.00
    D17    Rectangle 15.75 X 47.24  Rotation 90
    D18    Rectangle 39.37 X 42.91
    D24    Round 50.00
    D25    Round 25.00
    D26    Round 32.00
    D27    Round 48.00
    D28    Round 15.00
    D72    Round 56.00
    D99    Square 54.00
    D100   Round 54.00
    D101   Round 70.00
    D111   Square 60.00
    D112   Round 60.00
    D143   Rectangle 51.18 X 94.49
    D144   Rectangle 59.06 X 118.11
    D145   Rectangle 275.59 X 275.59  Rotation 90
    D146   Rectangle 9.84 X 15.75
    D147   Rectangle 55.00 X 83.00  Rotation 90
    D148   Round 7.00

Gerber Output
=============

H:\PrimerCube Tech Transfer\Printed Circuit Boards\PrimerCube MotherBoard V10 - Bottom Silkscreen.gbr

    Layers:
    ---------------------
    Bottom Silkscreen
    Board Outlines

    D-Code Shape  (thou)
    -----------------------
    D10    Round 1.00
    D11    Round 5.00
    D13    Round 6.00
    D149   Round 8.00
    D150   Round 9.84
    D151   Round 7.87

Gerber Output
=============

H:\PrimerCube Tech Transfer\Printed Circuit Boards\PrimerCube MotherBoard V10 - Bottom Documentation.gbr

    Layers:
    ------------------------
    Bottom Documentation
    Board Outlines

    D-Code Shape  (thou)
    -----------------------
    D10    Round 1.00
    D11    Round 5.00

Gerber Output
=============

H:\PrimerCube Tech Transfer\Printed Circuit Boards\PrimerCube MotherBoard V10 - Bottom Solder Mask.gbr

    Layers:
    ----------------------
    Bottom Solder Mask

    D-Code Shape  (thou)
    ------------------------------------------------
    D10    Rectangle 57.18 X 100.49
    D11    Rectangle 45.37 X 48.91
    D12    Square 60.00
    D13    Round 60.00
    D14    Round 76.00
    D15    Rectangle 65.06 X 124.11
    D16    Rectangle 281.59 X 281.59  Rotation 90
    D17    Rectangle 15.84 X 21.75
    D18    Rectangle 21.75 X 53.24  Rotation 90
    D19    Rectangle 61.00 X 89.00  Rotation 90
    D70    Square 66.00
    D71    Round 66.00

Gerber Output
=============

H:\PrimerCube Tech Transfer\Printed Circuit Boards\PrimerCube MotherBoard V10 - Bottom Paste Mask.gbr

    Layers:
    ---------------------
    Bottom Paste Mask

    D-Code Shape  (thou)
    ------------------------------------------------
    D20    Rectangle 45.18 X 88.49
    D21    Rectangle 33.37 X 36.91
    D22    Rectangle 53.06 X 112.11
    D23    Rectangle 269.59 X 269.59  Rotation 90
    D24    Rectangle 3.84 X 9.75
    D25    Rectangle 9.75 X 41.24  Rotation 90
    D26    Rectangle 49.00 X 77.00  Rotation 90

NC Drill Output
===============

H:\PrimerCube Tech Transfer\Printed Circuit Boards\PrimerCube MotherBoard V10 - Drill Data - Through Hole.drl

    Output:
    ---------------------------
    Plated Round Drill Holes
    Plated Slots
    Plated Board Outlines

    Tool  Size           Count   ID
    --------------------------------------
    T001  0.01600 inches 11    A
    T002  0.02400 inches 73    B
    T003  0.03200 inches 14    C
    T004  0.03400 inches 2     D
    T005  0.04000 inches 26    E
    --------------------------------------
    Total                126
    --------------------------------------

H:\PrimerCube Tech Transfer\Printed Circuit Boards\PrimerCube MotherBoard V10 - Drill Data - Through Hole (Unplated).drl

    Output:
    -----------------------------
    Unplated Round Drill Holes
    Unplated Slots
    Unplated Board Outlines

    Tool  Size           Count   ID
    --------------------------------------
    T001  0.02500 inches 1
    --------------------------------------
    Total                1
    --------------------------------------


Gerber Output
=============

H:\PrimerCube Tech Transfer\Printed Circuit Boards\PrimerCube MotherBoard V10 - Drill Ident Drawing - Through Hole.gbr

    Layers:
    ------------------
    [Through Hole]


Drill Ident Drawing
===================

    Drill Plated Size Shape ID
    -----------------------------------
    16    Y      100  Round A
    24    Y      100  Round B
    32    Y      100  Round C
    34    Y      100  Round D
    40    Y      100  Round E

    D-Code Shape  (thou)
    -----------------------
    D27    Round 100.00
    D28    Round 5.00

End Of Report.
